

**TEMPLATE PENYEDIAAN BAB DALAM BUKU**

***[CONTOH HALAMAN PRELIM/AWALAN UNTUK MANUSKRIP]***

**KANDUNGAN/CONTENTS**

(contoh susunan isi kandungan)

DEDIKASI/DEDICATION (*Jika ada*) …………………………

PENGHARGAAN/ACKNOWLEDGMENTS (*Jika ada*) …………………………

KATA PENGANTAR/FORWARD (*Jika ada*) …………………………

SENARAI PENYUMBANG/LIST OF CONTRIBUTORS …………………………

(*Perlu ada*)

PRAKATA/PREFACE (*Perlu ada*) …………………………

PENGENALAN/INTRODUCTION (*Perlu ada*) …………………………

BAB 1 …………………………

BAB 2 …………………………

dan seterusnya……………………… …………………………

BIODATA PENULIS *(Jika ada)* …………………………

RUJUKAN/REFERENCE *(Perlu ada)* …………………………

INDEKS/INDEX *(Perlu ada)* …………………………

**\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\***

**DEDIKASI/*DEDICATION***

*(Jika ada)*

Bahagian ini boleh dimasukkan jika perlu. Penulis boleh mendedikasikan dengan menujukan sesuatu kepada seseorang atau sesuatu sebagai tanda penghormatan atau kasih sayang. Jumlah kepanjangan paling minima dua halaman.

**PENGHARGAAN/*ACKNOWLEDGMENTS***

*(Jika ada)*

Bahagian ini boleh dimasukkan jika perlu. Penulis memberi pengiktirafan kepada seseorang berdasarkan sumbangan atau perkhidmatannya. Dalam konteks ini pengiktirafan di tempat kerja adalah penghargaan terhadap sumbangan atau perkhidmatan pekerja. Jumlah kepanjangan paling minima dua halaman.

**KATA PENGANTAR/*FORWARD***

*(Jika ada)*

Bahagian ini boleh dimasukkan jika perlu. Penulis boleh mendapatkan pakar-pakar, tokoh dalam bidang yang diperkatakan dalam buku untuk memberikan ulasan serta penulisan analisis yang mendalam tentang hal-hal dan isu utama yang dibicarakan dalam buku. Jumlah kepanjangan paling minima dua halaman.

**SENARAI PENYUMBANG/*LIST OF CONTRIBUTORS***

(*Perlu ada*)

Bahagian ini menyenaraikan nama dan institusi penyumbang buku dalam setiap bab dalam buku tersebut.

**PRAKATA/*PREFACE***

(*Perlu ada*)

Bahagian ini menjelaskan tentang latar belakang proses penulisan buku objektif permasalahan dan ruang lingkup yang diberi tumpuan oleh buku ini. Penulis boleh membuat ucapan dan memberi *highlight* kandungan utama. Seorang penulis yang baik mampu menghasilkan artikel yang menarik hasil ulasan bab-bab yang diulaskan.

**PENGENALAN/PENDAHULUAN/*INTRODUCTION***

(*Perlu ada*)

Bahagian ini mentakrifkan judul dan bidang buku tersebut, serta mengikat semua bab yang dihimpunkan.

## **TEMPLATE PENYEDIAAN MANUSKRIP**

***[CONTOH HALAMAN JUDUL UNTUK MANUSKRIP]***

**[ JUDUL MANUSKRIP - Saiz Rupa Taip 28 point ]**

**GREEN INFRASTRUCTURE**

**MATERIALS AND TECHNIQUES**

EDITORS

**Nor Hayati Abdul Hamid**

**Ahmad Kamil Arshad**

**Shamilah Anuar @ Anudai**

**[ Maksimum Editor tiga (3) orang ]**

###### [CONTOH Copyrights Page - PENERBIT UniMAP]

First Published 2023

© Universiti Malaysia Perlis 2023.

All rights reserved. No part of this book may be reproduced or transmitted in any forms by any means, electronic, mechanical, or otherwise, whether now or hereafter devised, including photocopying, recording, or by any information storage and retrieval system without express written prior permission from the Penerbit UniMAP.

CIP

ISBN 978-967-0922-XX-X

Published by: Penerbit UniMAP

Universiti Malaysia Perlis

No. 11 dan 12,

 Jalan Tiga, Pangkalan Jaya,

01000 Kangar, Perlis

Email: penerbitan@unimap.edu.my

Members of Malaysian Scholarly Publishing Council *- Majlis Penerbitan Ilmiah Malaysia* (MAPIM) Ministry of Higher Education Malaysia

Layout and Type Setting:

Penerbit UniMAP, Universiti Malaysia Perlis

Printing in Malaysia by: Sinaran Bros

Xxxxxxxx xxxxxxxx

Font: Candara Size: 10/12 pt

***[CONTOH HALAMAN BAHAGIAN ISI KANDUNGAN]***

**CONTENTS**

**LIST OF CONTRIBUTORS**

**PREFACE**

**INTRODUCTION**

|  |
| --- |
| **1****SURFACE TREATED RECYCLED CONCRETE AGGREGATE (RCA) AS GREEN CONSTRUCTION MATERIALS***Aiman Alodain, Ahmad Ruslan Mohd Ridzuan, Mohd Afiq Mohd Fauzi, Nor Hayati Abdul Hamid and Mohd Shafee Harun* |
| Introduction |
| Characteristics of RCA |
| Properties of RCA |
| High Performance RCA Concrete |
| Treatment of RCA |
| Conclusions and Recommendations |
| References |
| **2****USAGE OF RECYCLED CONCRETE FINES IN GREEN ENGINEERED CEMENTITIOUS COMPOSITES***Lee Siong Wee, Ahmad Ruslan Mohd Ridzuan, Fauzilah Ismail and Oh Chai Lian* |
| Introduction |
| Experimental Investigations |
| Test Results and Discussion |
| Conclusion |
| References |

***[CONTOH SENARAI PENYUMBANG/LIST OF CONTRIBUTORS]***

 [Saiz Rupa Taip 11 point]

**LIST OF CONTRIBUTORS**

Aiman Alodain

Faculty of Civil Engineering, Universiti Teknologi MARA, 40450 Shah Alam, Selangor, Malaysia

Ahmad Ruslan Mohd Ridzuan

Institute for Infrastructure Engineering and Sustainable Management (IIESM), Universiti Teknologi MARA, 40450 Shah Alam, Selangor, Malaysia

Mohd Afiq Mohd Fauzi

Faculty of Civil Engineering, Universiti Teknologi MARA, 40450 Shah Alam, Selangor, Malaysia

Nor Hayati Abdul Hamid

Institute for Infrastructure Engineering and Sustainable Management (IIESM), Universiti Teknologi MARA, 40450 Shah Alam, Selangor, Malaysia

Mohd Shafee Harun

Institute for Infrastructure Engineering and Sustainable Management (IIESM), Universiti Teknologi MARA, 40450 Shah Alam, Selangor, Malaysia

Lee Siong Wee

Faculty of Civil Engineering, Universiti Teknologi MARA Johor, Pasir Gudang Campus, 81750 Masai, Johor, Malaysia

***[CONTOH PRAKATA/PREFACE]***

**PREFACE**

This book presents research-based best practices related to green infrastructure by highlighting modern techniques and tools that integrate the invention technology. These approaches are based on the current problems in the construction industry. Concrete is a major material used in the construction industry and it has never been claimed as an environmentally friendly material because of its damaging nature resource consumption. This book emphasizes the Recycle Aggregate (RCA), fines concrete and POFA concrete as a construction material. Meanwhile, the existing pavement materials were also investigated for sustainable pavement by providing the alternative binder using charcoal ash from coconut shell. Furthermore, the innovative Wood-Wool Cement Board (WWCB) as a sustainable green infrastructure material.

 Chapter 1 - This review paper provides an inclusive summary of the use of RCA in concrete and an overview of its influence on the properties of RCA in concrete. It has been found that the mechanical and durability performance of RCA concrete is commonly lower compared to conventional concrete. The previous research showed that the reason for the poor quality of the RCA is the residual adhered mortar. This adhered mortar is reported as the main cause of the quality issue of RCA concrete. However, recent research showed the possibility to use the RCA in the production of concrete with very comparable mechanical and durability performance when surface treatment applied on the RCA. The use of the RCA as a substitute for the natural aggregate in concrete applications is limited to low or moderate grade concrete due to limited knowledge and experimentation on the HPC production. Thus, more research needs to be conducted on the surface treated RCA and its influence on the properties of high-performance concrete as compared to both HPC with untreated RCA and conventional HPC. Extending the application of RCA toward the production of HPC appears to be a promising contribution towards the sustainability of the environment and the industry.

 Chapter 2 - Compression test of Series 1 indicates that green ECC mixture with 70% of GGBS has shown enhancement in compressive strength over normal concrete. When the ratio of river sand to binder was fixed at 0.2, optimum compressive strength i.e. 90.3 MPa is attained when fiber 2.0% in volume fraction was employed. The use of RCF to replace river sand in ECC G70F2.5 yields slightly better result of compressive strength compared to its counterpart. Due to the limitation of this study, more research is needed to confirm the feasibility of using RCF to replace river sand in different fiber content.

 Chapter 3 - CIPR is an economical and environmentally sound alternative to conventional rehabilitation methods such as structural overlay or reconstruction. The reuse of existing pavement materials is a sustainable approach to pavement rehabilitation as new materials are conserved. Its use in Malaysia is expected to increase in the future as more pavement rehabilitation works instead of new roads construction will be carried out to preserve the integrity of the pavement structure and to extend the pavement life. However, an adequate understanding of the CIPR process, its suitability and limitations are essential for the correct pavement candidate to be chosen, for the works to be carried out successfully and for the pavement to perform satisfactorily.

Chapter 4 - The workability and compressive strength of normal concrete using POFA as partial cement replacement were investigated. Four types of mix design, including control design for concrete with normal strength of 30 N/mm2 at the age of 28 days. Replacement of cement by 5% of POFA produces equal compressive strength with concrete without POFA when the concrete reaches 28 days of age.

Chapter 5 - Good quality of pavement should have high structural integrity, which provides a strong, smooth, and safe riding surface for road users. In Malaysia, a common type of distress in asphalt pavement is permanent deformation. This study attempts to investigating NCA from coconut shell that is utilized as the main material in the bitumen modification. The effects of NCA on the bitumen subjected to numerous grinding times are evaluated, and the optimum grinding time that can produce the optimum NCA is determined. The optimum grinding time that showed the highest performance of bitumen was 30 h, which produced the optimum size of 148 nm. The incorporation of NCA increased the stiffness of the bitumen up to 47% and increased the softening point value by approximately 12% higher than the virgin binder. The PI values for the modified bitumen were not within the specified range, but the values did not exceed −2, except for the NCA0 and NCA5.

Chapter 6 - Poor performances of precast buildings during earthquakes were due to inadequate connections between the structure’s components, insufficient seating and anchorage and poor workmanship and quality materials used. It is important to investigate their seismic performance by conducting experimental work, analyzing the data and modelling them using nonlinear time history analysis of the earthquake’s excitations. The elastic stiffness is higher than secant stiffness for the single bay double-storey house, exterior beam-column joints with corbels and three-storey tunnel form buildings. Displacement ductility for all the three specimens are less than two (2) and to survive under earthquake attack, the ductility of the structure should be within the range from three (3) to six (6) as specified by the current seismic code of practice (EC8). Most of the failure mode occurred at the wall-beam joints, wall-foundation joints, beam-column joints, wall-slab joints and column-foundation joints where all the vertical loads and horizontal loads are meet at these points. It can be concluded that, single and double tunnel TFB with shear walls performed the best as compared to precast beam-column joint with corbel and precast shear-key wall panel.

Chapter 7 - Wood-cement composite which is a hybrid material that made from of cement and lignocellulosic material is gaining traction globally. Various studies are being conducted intensively to investigate its properties. In many parts of the word, it is also being manufactured industrially in the form of wall panels. To this day, conventional composite panels bonded by adhesive are manufactured in a greater volume than wood-cement composite. wood-cement composites are extremely useful especially in the prefabricated construction applications that utilize non-load bearing elements such as walls, ceiling and insulation panel. The developments of wood-cement hybrid composites which are low in cost have been regarded as a significant contribution to alleviate the housing problem faced by many developing countries.

***[CONTOH PENGENALAN/INTRODUCTION]***

**INTRODUCTION**

This book entitled ‘**Green Infrastructure Materials and Techniques**’ has been written in such a way that it will benefit the postgraduate and undergraduate students, supervisors, lecturers, construction industries and manufacturers. Human being produces a lot of waste such as food waste, agriculture waste, construction waste, industrial waste and chemical waste which harmful to the societies. Furthermore, these wastes need to through away on dumping site which is limited and could significantly impacts to the environments. One of the most excellent initiatives is to recycle these wastes into products that can be used by the societies toward clean and green environments.

 Recycle Concrete Aggregate (RCA) can be obtained from demolition buildings and dumping construction site. The RCA’s surface treatment can be done by soaking RCA into HCI solution which can improve the mechanical and physical properties of concrete. Green Engineered Cementitious Concrete (ECC) is made from cement, Ground Granulated Blast-Furnace Slag (GGBS), polypropylene fibers, water, superplasticizer and recycle sand from demolishing buildings. Cold In-Place Recycling (CIPR) is a pavement rehabilitation technique where the existing pavement materials are reused in-place along with additional virgin aggregates for the construction of the roads and highways. Palm Oil Fuel Ash (POFA) is a by-product waste from palm oil factories after burning the fibers and shell which used as partial replacement of cement. POFA can improve the compressive strength, porosity, tensile strength and superior filing ability in the concrete. Nano Charcoal Ash (NCA) is produced after burning the coconut shell and grinding it into the nano-size particles. NCA is used as an alternative binder in producing bitumen for pavement in construction of roads and highways.

 The recycle concrete aggregate and sand together with POFA as partial replacement of cement can be used as green infrastructure materials for the construction of structural elements such as precast wall panel, beam-column joint with corbels and tunnel form building as described in this book. Recycle aggregates from existing roads can use again using CIPR technique together with NCA as alternative binder for the construction of roads and highways. The wood wools can be obtained from debarked timber either from softwood or hardwood to make Wood-wool Cement Board (WWCB) which can be used as wall panels for the construction of houses, warehouses and shop lots.

 By using green recycle construction materials in developing and construction new houses and commercial buildings; we can sustain our environment for future generation. Therefore, our world will be become green, less emission of CO2, save from chemical waste, fresh atmosphere and hence reduce the global warming effects.

***[CONTOH HALAMAN BAHAGIAN TEKS]***

[Saiz Rupa Taip 12 point dan jenis taip Times News Roman/Arial]

**1**

 [Saiz Rupa Taip 12 point]

**SURFACE TREATED RECYCLED CONCRETE AGGREGATE (RCA) AS GREEN CONSTRUCTION MATERIAL**

**[Saiz Rupa Taip 14 point]**

*Aiman Alodain, Ahmad Ruslan Mohd Ridzuan, Mohd Afiq Mohd Fauzi, Nor Hayati Abdul Hamid and Mohd Shafee Harun*

**[Saiz Rupa Taip 10 point]**

* 1. **INTRODUCTION** [saiz 12pt, UPPERCASE, **bold**]

Concrete has never been claimed as an environmentally friendly material because of its damaging nature resource consumption and severe environmental impact after used. Nevertheless, it will remain one of the major construction materials being utilized worldwide for the construction of infrastructures, houses and commercial buildings. By taking the concept of sustainable development into consideration, the concrete industry has to be implemented at various strategies with regards to future used of concrete, for instance the recycle used of aggregate. In general, aggregates occupy about 55% to 80% of concrete volume of the constructed buildings. Without any proper alternative of aggregates being utilized for the year future, the concrete industry globally will consume about 8 to 12 billion tons annually of natural aggregates after the year 2010 (Tu *et al*., 2006). The large consumption of natural aggregates from the quarry will affect the environment and reduce the natural resources.

**1.1.1 Properties of RCA Concrete** [saiz 12pt, Capitalize Each Word, **bold**]

***1.1.1.1 Workability of RCA Concrete*** [saiz 12pt, Capitalize Each Word, **bold**, *italic*]

*1.1.1.1.1 Compressive Strength of RCA Concrete* [saiz 12pt, Capitalize Each Word, *italic*]

**[Bagi penggunaan sistem penomboran di atas digalakkan dalam bidang sains kejuruteraan, walau bagaimanapun, penggunaan sistem penomboran bergantung kepada kesesuaian manuskrip yang dihantar]**

***Contoh Penggunaan Rajah (Figure):***

|  |  |  |
| --- | --- | --- |
| https://cdnassets.hw.net/dims4/GG/419ca85/2147483647/resize/300x%3E/quality/90/?url=https%3A%2F%2Fcdnassets.hw.net%2Fa6%2F67%2Fbbe670d94a3e86e570473aadf6b1%2Ftmp97-2etmp-tcm45-628119.jpg | https://parkleasandsoil.com.au/wp-content/uploads/2015/02/20mm-rec-agg5-e1431059922168.jpg | https://parkleasandsoil.com.au/wp-content/uploads/2015/02/20mm-rec-agg2-150x150.jpg |

**Figure 1.1.** Three different types of recycle aggregates obtained from sites.

**[Saiz Rupa Taip 11 point]**

***Contoh Penggunaan Jadual (Table):***

**Table 1.1** Properties of the coarse aggregate (Thomas *et al*. 2013)

**[Saiz Rupa Taip 11 point]**

|  |  |
| --- | --- |
| **Property** | **Aggregate** |
| **NA (6/12)** | **NA (12/20)** | **RCA (6/20)** |
| Relative density of particle (g/cm3) | 2.51 | 2.54 | 2.32 |
| Density of particle saturated with dry surface (g/cm3) | 2.55 | 2.59 | 2.31 |
| Water absorption (wt. %) | 1.8 | 1.6 | 5.3 |

***[CONTOH RUJUKAN/REFERENCES]***

**[Rujukan diletakkan pada setiap akhir bab]**

**RUJUKAN/REFERENCES**

*(Perlu ada)*

Bahagian ini mentakrifkan senarai yang disediakan oleh penulis untuk memudahkan pembaca mendapatkan bahan-bahan tambahan. Rujukan ditulis/diberikan dalam gaya APA.

***Contoh:***

Contoh Rujukan: **BUKU**

Jalil,M. *et al*. (2013). *Semiconductor Optical Amplifiers and Related Applications*. Skudai: Penerbit UTM Press.

Contoh Rujukan: **JURNAL**

Nakamura S. and K. Tajima. 1997. “Experimental Investigations on High Speed Switching Characteristics of a Novel.” *Applied Physics Letter*, 65 (1): 283-455.

Contoh Rujukan: **PROSIDING/CONFERENCE**

Mecha, B. *et al*. 1998. Nonlinear Responds of a Spar in Deep Water”. Proceeding of the fifth International Offshore and Engineering Conference. The Netherlands, 11-15 June.

Contoh Rujukan: **TESIS**

King, K. 1987. “Development of Pressurised Systems for Oxidation Studies”. Unpublished ph.D. Thesis. Pennsylvania University.

Contoh Rujukan: **LAMAN SESAWANG/WEBSITE**

Global Security.org. 2016. “Tension Leg Platform technology”. Retrieved from http://www.globalsecurity.org/military/systems/ship/platform (accessed on 4 november 2017.

***[CONTOH HALAMAN AKHIRAN UNTUK MANUSKRIP]***

**INDEKS/INDEX**

*(Perlu ada)*

Entri daftar kata penting menurut abjad dan diletakkan di bahagian akhir buku.

***Contoh:***

**A**

advantages

aggregate

agricultural

apitong

asphalt pavements

**B**

beam-column interfaces

bitumen

bitumen emulsion

**C**

cement

coarse mixed aggregate

coconut shell

cold in-place recycling (CIPR)

compaction

compressive strength

concrete

consistency

construction

corbels

core samples

cracking

**BIODATA PENULIS**

*(Jika ada)*

|  |  |
| --- | --- |
| C:\Users\User\Downloads\WhatsApp Image 2020-06-02 at 3.14.04 PM.jpeg | Prof Dr Nor Hayati Abdul Hamid has been working as a lecturer at University Teknologi Mara, Shah Alam, Selangor for 26 years. She completed her PhD (Earthquake Engineering) from University of Canterbury, Christchurch, New Zealand in 2006. She received her Master of Science in Construction Management and Structural Engineering from University of NewCastle Upon Tyne, United Kingdom in 1993 and obtained her BSc (Civil Engineering) from University of Pittsburgh, United States of America in 1989. Her research interests’ fields are based-isolation system, seismic performance of precast buildings and tunnel form building under earthquake excitation, seismic performance of beam-column joints with corbel designed using BS8110 and Eurocode 8. She had published more than 200 articles in journals and conferences. |
|  | Assoc. Prof. Ir. Dr. Ahmad Kamil Arshad graduated PhD from Universiti Teknologi Mara, Shah Alam, MSc in Highway & Transportation from Universiti Putra Malaysia and BSc from Curtin University of Technology, Perth, Western Australia. He has about 20 years’ experience in the civil engineering industry with various organizations in Malaysia. His area of interest is the management, planning and design of highway systems, particularly in pavement engineering. His research focused on environmental-friendly and sustainable asphalt materials, pavement design and rehabilitation, sustainable transportation and traffic engineering. He is a Professional Engineer registered with the Board of Engineers and the Corporate Member of The Road Engineering Association of Malaysia and a Fellow of The Institution of Engineers, Malaysia (FIEM).  |